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	Anhydrous Ethanol Grade
	Characteristics & Purity
	Primary Export Applications

	1
	Bulk Fuel-Grade Anhydrous (99.6%)
	Standard dehydrated ethanol for automotive fuel blending.
	Automotive Fuel Blending

	2
	Pharmaceutical Grade Anhydrous (IP/BP/USP)
	Ultra-pure (>99.9%), free from trace impurities and heavy metals.
	Solvents for Active Pharmaceutical Ingredients (APIs), Vaccines

	3
	Electronic / Semiconductor Grade Anhydrous
	Extreme purity (99.99%), ultra-low particulate and moisture content.
	Semiconductor cleaning, Microchip manufacturing, PCBs

	4
	Cosmetic & Perfumery Grade Anhydrous
	Deodorized, absolute zero water to prevent clouding in luxury perfumes.
	Luxury Fragrances, Aerosol Cosmetics, Hair Sprays

	5
	Botanical & Nutraceutical Extraction Grade
	Food-safe anhydrous ethanol. Used as a clean solvent.
	Extracting CBD, Curcumin, Ashwagandha, and herbal resins



