	S.No.
	Biomass Product Type
	Characteristics & Processing
	Primary Export Application

	1
	Standard Industrial Bagasse Pellets (White Pellets)
	Raw, dried, and compressed sugarcane bagasse. Moderate calorific value (~3500-4000 kcal/kg).
	Power Plant Co-firing, Large Industrial Boilers

	2
	Torrefied Sugarcane Pellets (Bio-Coal / Black Pellets)
	Thermally treated (roasted) in an oxygen-deprived environment. High energy density (~5000 kcal/kg), water-resistant.
	Direct Coal Replacement, Steel Mills, Cement Plants

	3
	Sugarcane Trash / Leaf Pellets
	Made from harvested sugarcane tops and leaves left in the field.
	Lower-grade heating, small industrial furnaces

	4
	Blended Biomass Pellets (Bagasse + Mustard/Rice Husk)
	Bagasse mixed with other high-lignin agricultural residues for better binding and combustion.
	Textile mills, commercial heating, brick kilns

	5
	Premium Low-Ash Bagasse Pellets
	Highly purified bagasse, dust-extracted, extremely low ash (<2%).
	Residential pellet stoves, commercial space heating

	6
	Bagasse Briquettes (Industrial Logs)
	Larger form factor (60mm-90mm diameter) compressed biomass without binders.
	Heavy industrial furnaces, traditional kilns
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