	S.No.
	Bagasse Pulp Type
	Characteristics & Processing
	Primary  Applications

	1
	Molded Bagasse Pulp (Thermoformed Tableware)
	Fully processed, pressed into shapes (plates, bowls, clamshells). 100% biodegradable, PFAS-free.
	Food Service, QSR (Quick Service Restaurants), Retail Packaging

	2
	Bleached Bagasse Pulp (White Pulp)
	Chemically pulped and bleached to high brightness. Short-fiber structure.
	Tissue Paper, Printing & Writing Paper, Specialty Hygiene

	3
	Unbleached Kraft Bagasse Pulp (Brown Pulp)
	Chemically pulped without bleaching. High strength, natural brown color.
	Corrugated Boxes, Kraft Paper Bags, E-commerce Packaging

	4
	Dissolving Grade Bagasse Pulp
	Highly refined (>90% pure cellulose). Requires advanced chemical processing.
	Viscose / Rayon Textiles, Modal Fabrics, Cellophane

	5
	Chemi-Thermo-Mechanical Pulp (CTMP)
	Hybrid mechanical and chemical process. High yield, bulky.
	Absorbent cores, Paperboards, Folding Cartons

	6
	Bagasse Fluff Pulp
	Highly absorbent defibrated pulp. Competes with Southern Bleached Softwood Kraft (SBSK).
	Diapers, Sanitary Pads, Adult Incontinence Products
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